* Plate ID recorded
* Controls within expected Ct range
* Replicates within tolerance (e.g., SD ≤ 0.5 Ct)
* Melt curves inspected (no unexpected peaks)
* Outliers documented & rationale recorded